Rockville Center Well Information

4A (N-0072)

Coordinates: 40°41’05” N, 73°37’37” W

* Depth: 615 ft, 6 in below surface
* Screen Length: 60 ft
* Depth to top of Casing: 544 ft
  + **Screening Interval**: 544 ft – 604 ft
  + 11 ft, 6 in sump

4B (N-3745)

Coordinates: 40°41’05” N, 73°37’45” W

* Depth: 597 ft below surface
* Screen Length: 50 ft
* Depth to top of Casing: 542 ft
  + **Screening Interval**: 542 ft – 592 ft
  + 5 ft sump

4C (N-8218)

Coordinates: 40°41’04” N, 73°37’41” W

* Depth: 465 ft below surface
* Screen Length: 60 ft
* Depth to top of Casing: 400 ft
  + **Screening Interval**: 400 ft – 460 ft
  + 5 ft sump